Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-11-73
P. 64

    UF3J14E0.book  Page 59  Friday, June 23, 2017  9:47 AM

                            Equipment operation

                            To open the glove compartment:        To close the glove compartment:
                            Turn the glove compartment knob 90° to the  Lower the lid, and then turn the glove com-
                            left or right, and then lift up the lid.  partment knob to securely lock the lid in pla-
                                                                  ce.

                                         1

                              1 Glove compartment knob

                                                            1

                              1 Glove compartment
                                                                  To drain water from the glove compartment:
                              Glove compartment:                  (1) Remove the drain plug on the bottom of
                                Capacity:                            the glove compartment to drain the wa-
                                  7.0 L (1.8 US gal, 1.5 Imp.gal)    ter.
                                Load limit:
                                  1.0 kg (2 lb)

                                                                       1

                                                                   1 Drain plug
                                                                  (2) Securely install the drain plug in its origi-
                                                                     nal position.

                            59

| 59 60 61 62 63 64 65 66 67 68 69 |