Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-11-73
P. 66

    UF3J14E0.book  Page 61  Friday, June 23, 2017  9:47 AM

                            Equipment operation

                            Removable beverage holder             To open the built-in watertight storage com-
                            The removable beverage holder is located in  partment:
                            the glove compartment. (See page 58 for in-  Loosen the cap and remove it.
                            formation on the glove compartment.)
                                1

                                                                                     1

                                                                   1 Cap
                              1 Removable beverage holder
                            EJU42311
                            Watertight storage compartments
                            This model is equipped with a built-in water-
                            tight storage compartment and a removable
                            watertight storage compartment.
                            These compartments are watertight when
                            their caps are closed securely.
                            Built-in watertight storage compartment
                            The built-in watertight storage compartment    1
                            is located near the port (left) side of the multi-
                                                                   1 Built-in watertight storage compartment
                            function information center.
                                                                    Built-in watertight storage compart-
                                                                    ment:
                                                                      Capacity:
                                                                        2.5 L (0.7 US gal, 0.6 Imp.gal)
                                                                      Load limit:
                                                                        1.0 kg (2 lb)
                                                                  To close the built-in watertight storage com-
                                                                  partment:
                                                                  Securely install the cap by tightening it until it
                                                                  stops.
                                                                  Removable watertight storage compart-
                                                                  ment
                                                                  The removable watertight storage compart-
                                                                  ment is located under the rear seat.

                            61

| 61 62 63 64 65 66 67 68 69 70 71 |