Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-11-73
P. 45

    UF3J14E0.book  Page 40  Friday, June 23, 2017  9:47 AM

                                                                      Watercraft operation

                            EJU40001
                              Watercraft operation modes                                       “L-
                                                                   Number of   Low RPM Mode   MODE”
                                                                     beeps       operation   indicator
                            EJU36787                                                           light
                            Low RPM Mode
                                                                                              Comes
                            The Low RPM Mode is a function that limits           Activated
                                                                                                on
                            the maximum engine speed to approximately
                                                                                Deactivated   Goes off
                            70% of the maximum engine speed in  the
                            normal mode.                          TIP:
                            The Low RPM Mode can only be activated  If the remote control transmitter is operated
                            and deactivated  by operating  the remote  while the multifunction information center is
                            control transmitter that is included with this  in the standby state, the center performs the
                            watercraft. (See page 30 for information on  initial operation, and then the setting is se-
                            the remote control transmitter.)      lected.
                                                                  To activate the Low RPM Mode:
                                                                  Push the “L-Mode” (unlock) button on the re-
                                                                  mote control transmitter for more than 4 sec-
                                                                  onds. Once the beeper sounds three times
                                                                  and the “UNLOCK” indicator light  blinks
                                                                  three times, then comes on, the “L-MODE”
                                                                  indicator light comes on and the Low RPM
                                                                  Mode is activated.
                                                                  TIP:
                                                                  If the Low RPM Mode is activated immediate-
                              1 Remote control transmitter
                                                                  ly after the information display turns off, the
                            TIP:                                  “L-MODE” indicator light will not come on.
                            The Low RPM Mode can only be activated  The “L-MODE” indicator light will come  on
                            when the engine is  stopped in  the  unlock  when the engine is started.
                            mode of the Yamaha Security System.
                            Activating and deactivating the Low RPM        1  L-Mode
                            Mode                                                                2
                            Activation of the Low RPM Mode will be con-
                            firmed by the number of beeps when the re-
                            mote control transmitter is operated, and by
                            the “L-MODE” indicator light of the multifunc-
                            tion information center. (See page 44 for in-
                            formation on  the multifunction information
                            center.)
                                                                   1 “L-Mode” (unlock) button
                                                                   2 “L-MODE” indicator light

                                                                                                   40

| 40 41 42 43 44 45 46 47 48 49 50 |