Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-11-73
P. 57

    UF3J14E0.book  Page 52  Friday, June 23, 2017  9:47 AM

                                                                     Instrument operation

                            Fuel consumption per kilometer/mile   Air temperature (FX Cruiser SVHO / FX
                            This display shows the current fuel consump-  Limited SVHO)
                            tion in liters per kilometer “L/KM” or gallons  This display shows the ambient air tempera-
                            per mile “G/MILE”.                    ture “E TEMP” (environmental temperature).
                            TIP:
                            The  actual fuel consumption varies greatly
                            depending on the operating conditions. Use
                            this function as a reference only.

                                                                  Average speed/Tripmeter modes
                                                                  Average speed and distance traveled are re-
                                                                  corded once the “START/STOP” button is
                                                                  pushed to start the measurements, regard-
                                                                  less of the current display.
                            Water temperature (FX Cruiser SVHO / FX
                            Limited SVHO)                         TIP:
                            This display shows the ambient water tem-  The measurements are performed only while
                            perature “L TEMP” (lake temperature).  the engine is running.
                                                                  The measurements are not saved if the en-
                                                                  gine is stopped. The measurements are reset
                                                                  automatically when  the displays go off  25
                                                                  seconds after the engine stops.

                                                                                               1

                                                                                               2

                                                                   1 “START/STOP” button
                                                                   2 “MODE/RESET” button

                                                                                                   52

| 52 53 54 55 56 57 58 59 60 61 62 |