Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-11-73
P. 38

    UF3J14E0.book  Page 33  Friday, June 23, 2017  9:47 AM

                            Control function operation

                            in 5 seconds, release the start switch, wait 15  EJU31212
                                                                  Throttle lever
                            seconds, and then try again. NOTICE: Never
                                                                  The throttle lever increases the engine speed
                            push the start switch while the engine is
                                                                  when the lever is squeezed.
                            running. Do not operate the start switch
                            for  more than 5 seconds, otherwise the
                            battery will be discharged and the engine     1
                            will not start. Also, the starter motor could
                            be damaged. [ECJ01041]

                                                     1

                                                                   1 Throttle lever
                                                                  The throttle lever returns automatically to its
                                                                  fully closed (idle) position when released.
                                                                  EJU43342
                                                                  RiDE lever
                              1 Start switch
                                                                  When the RiDE lever is squeezed, the reverse
                            The engine will not start under any of the fol-  gate lowers and the watercraft starts moving
                            lowing conditions:                    in reverse. If the watercraft is moving forward,
                             Lock mode of the Yamaha Security System  the watercraft gradually slows down until it
                              has been  selected. (See page 31 for  stops, and then the watercraft starts moving
                              Yamaha Security System setting proce-  in reverse.
                              dures.)
                             Clip is removed  from  the engine  shut-off             1
                              switch.
                             Throttle lever is squeezed.
                             Throttle lever is malfunctioning.
                             RiDE lever is squeezed.
                             RiDE lever is malfunctioning.

                                                                   1 RiDE lever
                                                                  When the RiDE lever is released, it automati-
                                                                  cally returns to its fully closed (idle) position
                                                                  and the reverse gate moves to the neutral po-
                                                                  sition.

                            33

| 33 34 35 36 37 38 39 40 41 42 43 |