Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-11-73
P. 53

    UF3J14E0.book  Page 48  Friday, June 23, 2017  9:47 AM

                                                                     Instrument operation

                            TIP:                                  TIP:
                            The accuracy of the fuel level meter varies  Push any  of the  operation buttons  for the
                            depending on the operating conditions. Use  multifunction information center to stop the
                            this function as a reference only.    buzzer.
                                                                  EJU42271
                                                                  Oil pressure warning
                                                                  If the oil pressure drops significantly, the oil
                                                                  pressure warning indicator and the “WARN-
                                                                  ING” indicator  light blink, and the buzzer
                                                                  sounds intermittently. At the same time, the
                              1                                   engine speed is limited.

                              1 Fuel level meter
                            EJU42342
                            Fuel level warning
                            If the fuel remaining in the fuel tank drops to
                            about 18 L (4.8 US gal, 4.0 Imp.gal), the low-
                            est two fuel level segments, the fuel indicator,
                            and the “WARNING” indicator light blink, and
                            the buzzer sounds intermittently.     If the oil pressure warning is activated, imme-
                                                                  diately reduce the engine  speed,  return to
                                                                  shore, and then check the engine oil level.
                                                                  (See page 66 for information on checking the
                                                                  engine oil level.) If the oil level is sufficient,
                                                                  have a Yamaha dealer check the watercraft.
                                                                  TIP:
                                                                  Push any  of the  operation buttons  for the
                                                                  multifunction information center to stop the
                                                                  buzzer.
                                                                  EJU42371
                            If the fuel level warning is activated, refill the  Engine overheat warning
                                                                  If the engine temperature rises significantly,
                            fuel tank as soon as possible. (See page 64
                                                                  the engine overheat warning  indicator and
                            for information on filling the fuel tank.)
                                                                  the “WARNING” indicator light blink, and the
                            After the fuel tank is refilled, the warning sig-
                                                                  buzzer sounds intermittently. Then, the en-
                            nals will be cleared when  the engine  is  re-
                                                                  gine  overheat warning indicator and the
                            started.
                                                                  “WARNING” indicator light stop blinking and
                                                                  remain on, and the buzzer sounds continu-

                                                                                                   48

| 48 49 50 51 52 53 54 55 56 57 58 |