Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-11-73
P. 67

    UF3J14E0.book  Page 62  Friday, June 23, 2017  9:47 AM

                                                                     Equipment operation

                            To  open  the removable watertight storage  EJU42391
                                                                  Fire extinguisher holder and cover
                            compartment:
                                                                  The fire extinguisher holder and cover are lo-
                            (1) Remove the rear seat. (See page 54 for
                                                                  cated in the bow storage compartment.
                                seat removal and installation proce-
                                                                  To use the fire extinguisher holder and cover:
                                dures.)
                                                                  (1) Pull the hood latch rearward, and then lift
                            (2) Loosen the cap and remove it.
                                                                     up the rear of the hood.

                                                                                               1

                                    1

                              1 Cap
                                                                   1 Hood latch
                                                                  (2) Unhook the band and remove the fire ex-
                                                                     tinguisher cover.

                                                                             1
                                                                                 2

                                    1

                              1 Removable watertight storage compart-
                                ment
                              Removable watertight storage compart-  1 Fire extinguisher holder and cover
                              ment:                                2 Band
                                Capacity:
                                  9.0 L (2.4 US gal, 2.0 Imp.gal)  (3) Place the fire extinguisher in the holder,
                                Load limit:                          and then place the cover over the fire ex-
                                  3.0 kg (7 lb)                      tinguisher.
                                                                  (4) Securely fasten the cover and the fire ex-
                            To close the removable watertight storage
                                                                     tinguisher with the band.
                            compartment:
                                                                  (5) Push the rear of the hood down to se-
                            (1) Securely install the cap by tightening it
                                                                     curely lock it in place. Make sure that the
                                until it stops.
                            (2) Securely install the rear seat in its original
                                position.

                                                                                                   62

| 62 63 64 65 66 67 68 69 70 71 72 |