Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 98 - LIT-18626-11-73
P. 98

    UF3J14E0.book  Page 93  Friday, June 23, 2017  9:47 AM

                            Care and storage

                            EJU37146                              (4) Connect the garden hose  adapter to a
                                   Post-operation care
                                                                     garden hose.
                            EWJ00331
                                 WARNING
                            Always place the watercraft upright in a      1               2
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            After using the watercraft, always take it out
                            of the water, clean it, and store it. Leaving the
                            watercraft in the water for extended periods
                                                                   1 Garden hose adapter
                            will accelerate the rate of normal deteriora-
                                                                   2 Garden hose
                            tion of the jet pump and hull. Marine organ-
                            isms  and corrosion  are some of the  (5) Loosen the flushing hose connector cap
                            conditions that can shorten the life of many  and  remove  it. Insert the garden  hose
                            watercraft components.                   adapter into the flushing hose connector
                            EJU42771                                 by pushing and twisting it until it is se-
                            Flushing the cooling water passages      curely connected.
                            ECJ01880
                             NOTICE                                  3
                             Do not run the engine over 4000 r/min on
                              land. Also, do not run  the engine for
                              more than 15 seconds without supplying
                              water, otherwise the engine could over-
                              heat.                                                             1
                             Flush the cooling water passages to
                                                                                           2
                              prevent them from  clogging with salt,
                              sand, or dirt.
                                                                   1 Flushing hose connector
                            (1) Place the watercraft in a horizontal posi-
                                                                   2 Flushing hose connector cap
                                tion.
                                                                   3 Garden hose adapter
                            (2) Remove the seats and removable water-
                                                                  (6) Connect the garden hose to a water tap.
                                tight storage compartment. (See page 54
                                                                  (7) Make sure that the area around the wa-
                                for seat removal and installation proce-
                                                                     tercraft is  clear, and then  start the en-
                                dures and page 61 for information on the
                                                                     gine. Immediately after the engine starts,
                                removable watertight storage compart-
                                                                     fully turn the water supply on so that wa-
                                ment.)
                            (3) Open the stern  storage compartment.
                                (See page 60 for information on the stern
                                storage compartment.)

                            93

| 93 94 95 96 97 98 99 100 101 102 103 |