Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-11-73
P. 58

    UF3J14E0.book  Page 53  Friday, June 23, 2017  9:47 AM

                            Instrument operation

                            To start the measurements:
                            Push the “START/STOP” button for less than
                            1 second. The beeper sounds once and the
                            measurements start.
                            To stop the measurements:
                            Push the “START/STOP” button for less than
                            1 second while the measurements are being
                            recorded. The beeper sounds once and the
                            measurements stop.
                            To restart the measurements:
                            Push the “START/STOP” button for less than
                            1 second while the measurements are
                            stopped. The beeper sounds once and the
                            measurements restart.
                            To reset the measurements:
                            Push the “MODE/RESET” button for at least
                            2  seconds  while the measurements are
                            stopped. The beeper sounds twice and the
                            measurements are reset.

                            53

| 53 54 55 56 57 58 59 60 61 62 63 |