Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 87 - LIT-18626-11-74
P. 87

    UF2W14E0.book  Page 82  Thursday, June 15, 2017  11:29 AM

                                                                                      Operation

                            EJU40242
                            After removing the watercraft from
                            the water
                            ECJ01311
                             NOTICE
                            Do not run the engine over 4000 r/min on
                            land. Also, do not run the engine for more
                            than 15 seconds without supplying water,
                            otherwise the engine could overheat.
                            After operating and removing the watercraft
                            from the water, promptly discharge the  re-
                            maining water  from the cooling water  pas-
                            sages.
                            To discharge  water from the  cooling water
                            passages:
                            (1) Make sure that the area around the wa-
                                tercraft is clear, and then start  the en-
                                gine.
                            (2) Discharge the remaining water out of the
                                cooling  water passages by  alternately
                                squeezing and releasing the throttle lever
                                quickly for 10 to 15 seconds.
                            (3) Stop the engine.

                                                                                                   82

| 82 83 84 85 86 87 88 89 90 91 92 |