Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - LIT-18626-11-74
P. 60

    UF2W14E0.book  Page 55  Thursday, June 15, 2017  11:29 AM

                            Operation and handling requirements

                            (5) Loosen the fuel filler cap and remove it.  Do not  leave the watercraft with  a full
                                                                     tank in direct sunlight.
                                             1
                                                                                         1
                                                                                            2

                              1 Fuel filler cap
                            (6) Slowly add fuel to the fuel tank.  1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                              Fuel tank capacity:                    fuel tank
                                70 L (18.5 US gal, 15.4 Imp.gal)
                                                                                            1
                                                                                                 2

                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                            (7) Stop filling  when the  fuel level reaches  fuel tank
                                approximately 50 mm (2 in) from the top  (8) Wipe up any spilled fuel immediately with
                                of the fuel tank. Do not overfill the fuel  a dry cloth.
                                tank. Because fuel expands when it  (9) Securely install the fuel filler cap by tight-
                                heats up, heat from the engine or the sun  ening it until it clicks.
                                can cause fuel to spill out of the fuel tank.  (10) Return the hood to its original position,
                                                                     and then push the hood latch down to
                                                                     securely lock it in place. Make sure that
                                                                     the fuel filler cap and the hood are se-

                            55

| 55 56 57 58 59 60 61 62 63 64 65 |