Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 94 - LIT-18626-11-74
P. 94

    UF2W14E0.book  Page 89  Thursday, June 15, 2017  11:29 AM

                            Maintenance

                            (3) Lift up the engine cover to remove it.

                                                        1

                              1 Engine cover
                            To install the engine cover:
                            (1) Place the engine cover in its original po-
                                sition, and then push it down.

                            (2) Install the engine cover screws, and then
                                tighten them to the specified torque.
                              Tightening torque:
                                Engine cover screw:
                                  4.5 N·m (0.46 kgf·m, 3.3 lb·ft)
                            (3) Securely install the seats in their original
                                positions.

                            89

| 89 90 91 92 93 94 95 96 97 98 99 |