Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-11-74
P. 53

    UF2W14E0.book  Page 48  Thursday, June 15, 2017  11:29 AM

                                                                     Equipment operation

                            (3) Pull the seat rearward and remove it.  EJU31364
                                                                  Handgrip
                                                                  The handgrip is used when boarding the wa-
                                                                  tercraft from the water and when the spotter
                                                                  is facing rearward. WARNING! Do not use
                                                                  the handgrip to lift the watercraft.  The
                                                                  handgrip is not  designed to support the
                                                                  watercraft’s weight. If the handgrip
                                                                  breaks, the watercraft could  fall, which
                                                                  could result in severe injury. [EWJ00022]

                            To install the front seat:                                       1
                            (1) Insert the projection on the front of the
                                seat into the stay on the deck.

                                                                   1 Handgrip
                                                                  EJU34865
                                                                  Reboarding step
                                                                  The reboarding step is used to assist in re-
                                                                  boarding the watercraft from the water.
                            (2) Push the rear of the seat down to secure-  When boarding the watercraft, push the re-
                                ly lock it in place.              boarding step down until it stops. The step
                                                                  returns automatically to its original position
                                                                  when released. WARNING! Do not use the
                                                                  reboarding step to lift the watercraft. The
                                                                  reboarding step is not designed to support
                                                                  the watercraft’s weight. If the reboarding

                            (3) Securely install the rear seat in its original
                                position.

                                                                                                   48

| 48 49 50 51 52 53 54 55 56 57 58 |