Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-11-74
P. 85

    UF2W14E0.book  Page 80  Thursday, June 15, 2017  11:29 AM

                                                                                      Operation

                              from objects—you need  throttle  to    place both feet on the floor of the foot-
                              steer.                                 well.
                            ECJ01341
                             NOTICE
                            Never run the engine in water that is less
                            than 60 cm (2 ft) deep from the bottom of
                            the watercraft, otherwise pebbles or sand
                            could be sucked into the jet intake, caus-
                            ing impeller damage and engine overheat-
                            ing.

                                                                  (4) Look  in all directions, start  the  engine,
                                                                     and then start off slowly.
                                                                  EJU44210
                                                                  Capsized watercraft
                                                                  EWJ00672
                                                                      WARNING
                                                                  Improper uprighting can cause injury.
                                                                   Be sure to shut the engine off by pulling
                                                                   on the engine shut-off cord (lanyard) to
                                                                   remove the clip from the engine shut-off
                            EJU43271
                            Starting off from a trailer            switch.
                            (1) Launch the watercraft.             Do not put your hands in the intake
                            (2) Attach the engine shut-off cord (lanyard)  grate.
                                to your left wrist, and then attach the clip
                                                                  If the watercraft capsizes, turn it over imme-
                                to the engine shut-off switch.
                                                                  diately.
                            (3) Look in all directions, and then start the
                                                                  To upright the watercraft:
                                engine.
                                                                  (1) Remove the clip from the engine shut-off
                            (4) Squeeze the RiDE lever and  move the
                                                                     switch.
                                watercraft back slowly. (See page 36 for
                                                                  (2) Swim to the rear of the watercraft. Turn
                                RiDE lever operation procedures.)
                                                                     the watercraft over by pulling on the ride
                            EJU33114
                            Boarding and starting off from a dock    plate with one hand while pushing down
                            (1) Board the watercraft from the side.
                            (2) Attach the engine shut-off cord (lanyard)
                                to your left wrist, and then attach the clip
                                to the engine shut-off switch.
                            (3) Push the watercraft away from the dock,
                                grip the handlebars with both hands, and

                                                                                                   80

| 80 81 82 83 84 85 86 87 88 89 90 |