Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-11-74
P. 46

    UF2W14E0.book  Page 41  Thursday, June 15, 2017  11:29 AM

                            Watercraft operation

                            The “L-MODE” indicator light will come on
                            when the engine is started.

                                                1  L-Mode

                              1 “L-Mode” (unlock) button

                                      1             2

                              1 “UNLOCK” indicator light
                              2 “L-MODE” indicator light
                            To deactivate the Low RPM Mode:
                            Push the “L-Mode” (unlock) button on the re-
                            mote control transmitter for more than 4 sec-
                            onds. Once the beeper sounds two times and
                            the “UNLOCK” indicator  light blinks  two
                            times, then comes on, the “L-MODE” indica-
                            tor light goes off and the Low RPM Mode is
                            deactivated. When the Low RPM Mode is de-
                            activated, the watercraft returns to the nor-
                            mal operation mode.

                            41

| 41 42 43 44 45 46 47 48 49 50 51 |