Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - LIT-18626-11-74
P. 41

    UF2W14E0.book  Page 36  Thursday, June 15, 2017  11:29 AM

                                                                      Watercraft operation

                            EJU40014                                 reverse, and the “R” (reverse) shift indi-
                             Watercraft operation functions
                                                                     cator will be displayed.
                            EJU43154
                            Shift system                                              1
                            EWJ01773
                                 WARNING
                             Make sure that there are no obstacles or
                              people behind you before  shifting  into
                              reverse.
                             Do not touch the reverse gate while the
                              RiDE lever is being operated, otherwise
                              you could be pinched.
                                                                   1 RiDE lever
                             If the RiDE  lever and throttle lever are
                              being operated at the same time, do not
                              release only the RiDE lever. Otherwise,
                              the watercraft  could accelerate more
                              quickly than expected, which may lead
                              to an accident.                                     1
                            The RiDE lever and throttle lever can be oper-
                            ated to change the forward or rearward
                            movement of the watercraft only when the                            2
                            engine is running.  When the  RiDE  lever is
                            squeezed, the reverse gate lowers and de-  1 Reverse gate
                            flects the water jet being discharged from the  2 Reverse position
                            jet thrust nozzle so that the watercraft moves
                            in reverse or is in neutral. When the throttle le-
                            ver is squeezed, the reverse gate rises and
                            the watercraft moves forward.
                            TIP:
                             This  model is equipped with a function
                              which limits the engine speed in reverse.
                             When the  engine is started,  the reverse
                              gate automatically moves to the neutral po-
                              sition.                                              1
                            To shift into reverse:                 1 “R” (Reverse position)
                            (1) Release the throttle lever.       To shift into neutral from reverse:
                            (2) Squeeze the  RiDE lever. The reverse  Release the RiDE lever. The reverse gate will
                                gate will lower, the engine speed will in-  automatically return to the  neutral position
                                crease, the watercraft will start moving in

                                                                                                   36

| 36 37 38 39 40 41 42 43 44 45 46 |