Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-11-74
P. 62

    UF2W14E0.book  Page 57  Thursday, June 15, 2017  11:29 AM

                            Operation and handling requirements

                            (2) Remove the seats. (See page 47 for seat  (6) Loosen the engine oil filler cap and re-
                                removal and installation procedures.)  move it.
                            (3) Remove the dipstick and wipe it clean.

                                                                      1
                                                   1

                                                                   1 Engine oil filler cap
                              1 Dipstick
                                                                  (7) Slowly add engine oil.
                            (4) Insert the dipstick back into the dipstick  TIP:
                                tube  completely. Remove the  dipstick  The difference between the minimum and
                                again and make sure that the engine oil  maximum level marks on the dipstick is equal
                                level is between the minimum and maxi-  to approximately 1 L (1.06 US qt, 0.88 Imp.qt)
                                mum level marks.                  of engine oil.
                                                                  (8) Wait approximately 5 minutes to allow
                                                                     the engine oil to settle, and then check
                                                                     the engine oil level again.
                                                                  (9) Repeat steps 3–8 until the engine oil is at
                                                     1               the proper level.
                                                                  (10) Securely install the engine oil filler cap by
                                                     2
                                                                     tightening it until it stops.
                                                                  (11) Securely install the seats in their original
                                                                     positions.

                              1 Maximum level mark
                              2 Minimum level mark
                            (5) If the  engine oil  level is significantly
                                above the maximum level mark, consult
                                a Yamaha dealer. If the engine oil level is
                                below the minimum level mark, add en-
                                gine oil.

                            57

| 57 58 59 60 61 62 63 64 65 66 67 |