Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-11-75
P. 50

    UF4G12E0.book  Page 45  Tuesday, August 1, 2017  10:17 AM

                            Instrument operation

                                                                  EJU43720
                            TIP:                                  Oil pressure warning
                            The accuracy of the fuel level meter varies  If the oil pressure drops significantly, the oil
                            depending on the operating conditions. Use  pressure warning indicator, the check engine
                            this function as a reference only.    warning indicator, and the “WARNING” indi-
                                                                  cator light blink, and the buzzer sounds inter-
                                                                  mittently for 30 seconds. At the same time,
                                                                  the maximum engine speed is limited.

                                           1
                              1 Fuel level meter
                            EJU44020
                            Fuel level warning
                            If the fuel remaining in the fuel tank drops to
                            about 18 L (4.8 US gal, 4.0 Imp.gal), the low-  If the oil pressure warning is activated, imme-
                            est  two fuel level segments, the fuel level  diately reduce the engine  speed,  return to
                            warning indicator, and the “WARNING” indi-  shore, and then check the engine oil level.
                            cator light blink, and the buzzer sounds inter-  (See page 57 for information on checking the
                            mittently for 30 seconds.             engine oil level.) If the oil level is sufficient,
                                                                  have a Yamaha dealer check the watercraft.
                                                                  EJU43901
                                                                  Engine overheat warning
                                                                  If the engine temperature rises significantly,
                                                                  the engine overheat warning indicator, the
                                                                  check engine warning indicator, and  the
                                                                  “WARNING” indicator light blink,  and the
                                                                  buzzer sounds intermittently. After 5 sec-
                                                                  onds, the engine overheat warning indicator
                                                                  and the “WARNING”  indicator light stop
                                                                  blinking and  remain on,  and the buzzer
                            If the fuel level warning is activated, refill the  sounds continuously. After 30 seconds, the
                            fuel tank as soon as possible. (See page 55  buzzer stops. While the engine overheat
                            for information on filling the fuel tank.)
                            After the fuel tank is refilled, the warning sig-
                            nals will be cleared when  the engine  is  re-
                            started.

                            45

| 45 46 47 48 49 50 51 52 53 54 55 |