Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 55 - LIT-18626-11-75
P. 55

    UF4G12E0.book  Page 50  Tuesday, August 1, 2017  10:17 AM

                                                                     Equipment operation

                            step  breaks,  the watercraft could fall,  towing it in an emergency. (See page 100 for
                            which could result in severe injury. [EWJ01212]  information on towing the watercraft.)

                              1
                                                                       1

                              1 Reboarding step                    1 Bow eye
                                                                  EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                                                                  it.

                            ECJ00743
                             NOTICE
                            Use the reboarding step only to board the
                            watercraft in the water. Do not use the re-    1
                            boarding step for any other purpose. The  1 Stern eye
                            watercraft can be damaged.
                                                                  EJU40423
                                                                  Cleat
                            EJU34873
                            Bow eye                               The cleat is used to attach a ski rope to the
                            The bow eye is used to attach a rope to the  watercraft  when pulling a wakeboarder or
                            watercraft when transporting, mooring, or  water-skier.  WARNING! Do not use the
                                                                  cleat to lift the watercraft. The cleat is not
                                                                  designed to support the watercraft’s
                                                                  weight. If the cleat breaks, the watercraft

                                                                                                   50

| 50 51 52 53 54 55 56 57 58 59 60 |