Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 71 - LIT-18626-11-75
P. 71

    UF4G12E0.book  Page 66  Tuesday, August 1, 2017  10:17 AM

                                                                    Pre-operation checks

                            aged, obstructed, or not connected prop-  whole range, and that the free play is not ex-
                            erly. [EWJ00452]                      cessive.
                             1          2

                                        3

                              1 Negative (–) battery terminal: Black lead
                                                                  Turn the handlebars as far as possible to the
                              2 Positive (+) battery terminal: Red lead
                                                                  right and left to make sure that the jet thrust
                              3 Breather hose
                                                                  nozzle moves as the handlebars are turned,
                            Make sure  that the electrolyte level  is be-  and that there is no difference between the
                            tween the minimum and maximum level
                            marks. WARNING! Never operate the wa-
                            tercraft if the battery does not have suffi-
                            cient  power to start the engine or if it
                            shows any other signs of decreased pow-
                            er. Loss of battery power may leave you
                            stranded. [EWJ01241]

                              1 Maximum level mark
                              2 Minimum level mark
                            Make sure that the battery is securely held in
                            place.
                            EJU32614
                            Steering system checks
                            Turn the handlebars to the right and left sev-
                            eral times  to make sure that  operation is
                            smooth and  unrestricted throughout  the

                                                                                                   66

| 66 67 68 69 70 71 72 73 74 75 76 |