Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-11-75
P. 75

    UF4G12E0.book  Page 70  Tuesday, August 1, 2017  10:17 AM

                                                                    Pre-operation checks

                            Securely install the stern drain plugs by tight-  running. (See page 34 for information on the
                            ening them until they stop.           cooling water pilot outlet.)

                                           1

                              1 Stern drain plug
                                                                  EJU32715
                                                                  Multifunction information center check
                            EJU43810
                            Hood check                            Make sure that the multifunction information
                            Push down the hood latch and make sure  center operates properly. (See page 43 for in-
                            that it is securely closed.           formation on proper operation of the multi-
                                                                  function information center.)

                            EJU40146
                            Post-launch checks
                                                                  EJU43392
                            Perform the post-launch checks in the pre-  Shift system check
                            operation checklist while the watercraft is in  Operate the throttle lever and RiDE lever, and
                            the water and the engine is running.  check that the watercraft moves or does not
                            To perform the post-launch checks:    move according to the displayed shift indica-
                            (1) Launch the watercraft. (See page 73 for  tor. (See page 36 for shift system operation
                                information on launching the watercraft.)  procedures.)  WARNING! To avoid colli-
                            (2) Perform the checks and make sure that  sions, operate at safe speeds and keep a
                                there are no malfunctioning items or oth-
                                er problems.
                            EJU40553
                            Cooling water pilot outlet check
                            Make sure that water is discharged from the
                            cooling water pilot outlet while the engine is

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |