Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - LIT-18626-11-75
P. 76

    UF4G12E0.book  Page 71  Tuesday, August 1, 2017  10:17 AM

                            Pre-operation checks

                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]

                                                             2

                                                             3

                                                             4
                                             1
                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)
                            EJU40172
                            Engine idling speed check
                            Start the engine and warm it up. Use the ta-
                            chometer in the multifunction  information
                            center to make  sure  that the engine  idling
                            speed is not significantly above or below the
                            specified range.

                              Engine idling speed:
                                1500 ±100 r/min

                            71

| 71 72 73 74 75 76 77 78 79 80 81 |