Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-11-75
P. 44

    UF4G12E0.book  Page 39  Tuesday, August 1, 2017  10:17 AM

                            Watercraft operation

                                                                  The “L-MODE” indicator light will come  on
                                                          “L-
                              Number of   Low RPM Mode   MODE”    when the engine is started.
                                beeps       operation   indicator
                                                         light
                                                         Comes
                                            Activated
                                                          on
                                                                                      1  L-Mode
                                           Deactivated  Goes off
                            TIP:
                            If the remote control transmitter is operated
                            while the multifunction information center is
                            in the standby state, the center performs the
                            initial operation, and then the setting is se-
                                                                   1 “L-Mode” (unlock) button
                            lected.
                            To activate the Low RPM Mode:                   1             2
                            Push the “L-Mode” (unlock) button on the re-
                            mote control transmitter for more than 4 sec-
                            onds. Once the beeper sounds three times
                            and the “UNLOCK” indicator light blinks
                            three times, then comes on, the “L-MODE”
                            indicator light comes on and the Low RPM
                            Mode is activated.
                            TIP:
                            If the Low RPM Mode is activated immediate-  1 “UNLOCK” indicator light
                            ly after the information display turns off, the  2 “L-MODE” indicator light
                            “L-MODE” indicator light will not come on.
                                                                  To deactivate the Low RPM Mode:
                                                                  Push the “L-Mode” (unlock) button on the re-
                                                                  mote control transmitter for more than 4 sec-
                                                                  onds. Once the beeper sounds two times and
                                                                  the “UNLOCK”  indicator  light blinks two
                                                                  times, then comes on, the “L-MODE” indica-
                                                                  tor light goes off and the Low RPM Mode is
                                                                  deactivated. When the Low RPM Mode is de-
                                                                  activated, the watercraft returns to the nor-
                                                                  mal operation mode.
                                                                  EJU42484
                                                                  No-wake mode (VX Deluxe /
                                                                  VX Cruiser / VX Limited)
                                                                  The no-wake mode is a function that main-
                                                                  tains the engine speed at a fixed setting for
                                                                  operating the watercraft at low speeds. This
                                                                  function can be used only for forward water-

                            39

| 39 40 41 42 43 44 45 46 47 48 49 |