Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-11-75
P. 62

    UF4G12E0.book  Page 57  Tuesday, August 1, 2017  10:17 AM

                            Operation and handling requirements

                                curely closed before using  the  water-  EJU40291 Engine oil requirements
                                craft.
                                                                  EJU43960
                                                                  Engine oil
                                                                  ECJ00282
                                                                  NOTICE
                                                                  Use only 4-stroke engine oil. Usage of 2-
                                                                  stroke engine oil could result in severe en-
                                                                  gine damage.

                                                                    Recommended engine oil:
                                                                      YAMALUBE 4W
                                                                    Recommended engine oil type:
                                                                      SAE 10W-30, 10W-40, 20W-40,
                            (11) Securely install the seats in their original  20W-50
                                positions.                          Recommended engine oil grade:
                                                                      API SG, SH, SJ, SL

                                                                  Checking the engine oil level
                                                                  EWJ00341
                                                                      WARNING
                                                                  Engine oil is extremely hot immediately af-
                                                                  ter the engine is turned off. Coming in con-
                                                                  tact with or getting any engine oil on your
                                                                  clothes could result in burns.
                                                                  ECJ00392
                                                                  NOTICE
                                                                   Do not run the engine with too much or
                                                                   not enough oil in the oil tank, otherwise
                                                                   the engine could be damaged.
                                                                   Make sure that debris and water do not
                                                                   enter the oil tank filler hole. Debris and
                                                                   water in the engine oil can cause serious
                                                                   engine damage.

                                                                  TIP:
                                                                   When checking the engine oil level on land,
                                                                   the engine must be running while water is
                                                                   being supplied to the cooling water pas-
                                                                   sages. (See “Flushing  the cooling  water
                                                                   passages” on page 84 for information on
                                                                   supplying water.)

                            57

| 57 58 59 60 61 62 63 64 65 66 67 |