Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 58 - LIT-18626-11-75
P. 58

    UF4G12E0.book  Page 53  Tuesday, August 1, 2017  10:17 AM

                            Equipment operation

                            To close the glove compartment:       (2) Loosen the cap and remove it.
                            Push the lid down to securely lock it in place.
                                                                                  1

                                                                   1 Cap
                            EJU37235
                            Removable watertight storage compart-            1
                            ment
                            The removable watertight storage compart-
                            ment is located under the rear seat.
                            The compartment is watertight when the cap
                            is closed securely.
                            To  open  the removable watertight storage
                            compartment:
                            (1) Remove the rear seat. (See page 48 for
                                seat removal and installation proce-
                                                                   1 Removable watertight storage compart-
                                dures.)                              ment
                                                                    Removable watertight storage compart-
                                                                    ment:
                                                                      Capacity:
                                                                        5.8 L (1.5 US gal, 1.3 Imp.gal)
                                                                      Load limit:
                                                                        3.0 kg (7 lb)

                                                                  To close the removable watertight storage
                                                                  compartment:
                                                                  (1) Securely install the cap by tightening it
                                                                     until it stops.
                                                                  (2) Securely install the rear seat in its original
                                                                     position.
                                                                  EJU43790
                                                                  Fire extinguisher holder and cover
                                                                  The fire extinguisher holder and cover are lo-
                                                                  cated in the bow storage compartment.

                            53

| 53 54 55 56 57 58 59 60 61 62 63 |