Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 96 - LIT-18626-11-76
P. 96

    UF3Y11E0.book  Page 91  Tuesday, May 23, 2017  9:23 AM

                            Specifications

                            EJU34543                                Spark plug (NGK):
                                      Specifications                  CR9EB
                            Watercraft capacity:                    Spark plug gap:
                              Maximum people on board:                0.7–0.8 mm (0.028–0.031 in)
                                3 person                            Battery capacity:
                              Maximum load capacity:                  12 V, 19 Ah
                                220 kg (486 lb)                     Charging system:
                            Dimensions and weight:                    Flywheel magneto
                              Length:                             Drive unit:
                                3130 mm (123.2 in) (EX)             Propulsion system:
                                3140 mm (123.6 in) (EX Sport / EX Deluxe)  Jet pump
                              Width:                                Jet pump type:
                                1130 mm (44.5 in)                     Axial flow, single stage
                              Height:                               Impeller rotation:
                                1150 mm (45.3 in)                     Counterclockwise
                              Dry weight:                           Jet thrust nozzle angle:
                                262 kg (578 lb) (EX)                  24+24 °
                                265 kg (584 lb) (EX Sport)        Fuel and oil:
                                272 kg (600 lb) (EX Deluxe)         Recommended fuel:
                            Performance:                              Regular unleaded gasoline
                              Maximum fuel consumption:             Minimum octane rating (PON):
                                28.5 L/h (7.5 US gal/h, 6.3 Imp.gal/h)  86
                              Cruising range at full throttle:      Minimum octane rating (RON):
                                1.75 hour                             90
                              Trolling speed:                       Recommended engine oil:
                                1500 ±100 r/min                       YAMALUBE 4W or 4-stroke motor oil
                            Engine:                                 Recommended engine oil type SAE:
                              Engine type:                            SAE 10W-30, 10W-40, 20W-40, 20W-50
                                Liquid cooled 4-stroke, DOHC        Recommended engine oil grade API:
                              Number of cylinders:                    API SG, SH, SJ, SL
                                3                                   Fuel tank total capacity:
                              Engine displacement:                    50 L (13.2 US gal, 11.0 Imp.gal)
                                1049 cm³                            Engine oil quantity with oil filter replacement:
                              Bore × stroke:                          3.4 L (3.59 US qt, 2.99 Imp.qt)
                                82.0 × 66.2 mm (3.23 × 2.61 in)     Engine oil quantity without oil filter replacement:
                              Compression ratio:                      3.2 L (3.38 US qt, 2.82 Imp.qt)
                                11.0 : 1                            Engine oil total quantity:
                              Valve clearance-intake (cold):          3.7 L (3.91 US qt, 3.26 Imp.qt)
                                0.15–0.22 mm (0.0059–0.0087 in)
                              Valve clearance-exhaust (cold):
                                0.26–0.32 mm (0.0102–0.0126 in)
                              Lubrication system:
                                Dry sump
                              Cooling system:
                                Water
                              Starting system:
                                Electric
                              Ignition system:
                                T.C.I.

                            91

| 91 92 93 94 95 96 97 98 99 100 101 |