Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-11-76
P. 67

    UF3Y11E0.book  Page 62  Tuesday, May 23, 2017  9:23 AM

                                                                    Pre-operation checks

                            whole range. Also, make sure that the RiDE  falls off, allowing the watercraft to conti-
                            lever returns automatically to its fully closed  nue to run and cause an accident. [EWJ01221]
                            position when released.

                                                                  EJU40692
                                                                  Switch checks
                            EJU42181
                            Throttle lever checks                 ECJ01311
                            Operate the throttle lever  several times  to  NOTICE
                            make sure that operation is smooth through-  Do not run the engine over 4000 r/min on
                            out the whole range. Also, make sure that the  land. Also, do not run the engine for more
                            throttle lever returns automatically to its fully  than 15 seconds without supplying water,
                            closed (idle) position when released.  otherwise the engine could overheat.

                                                                  Check the start switch, the engine stop
                                                                  switch,  and the engine  shut-off switch  for
                                                                  proper operation. (See pages 30 to 30 for in-
                                                                  formation on operating each switch.)
                                                                                    1

                                                                                              3

                                                                                              4
                            EJU32664
                            Engine shut-off cord (lanyard) check
                            Make sure that the engine shut-off cord (lan-
                            yard) is not damaged. If the cord is damaged,        2        5
                            replace it.  WARNING! Never try to repair
                            the engine shut-off cord (lanyard) or tie it  1 Start switch
                                                                   2 Engine stop switch
                            together. The engine  shut-off cord (lan-
                                                                   3 Engine shut-off switch
                            yard) may not pull free when the operator
                                                                   4 Clip
                                                                   5 Engine shut-off cord (lanyard)
                                                                  To check the operation of the switches:
                                                                  (1) Push the start switch to make sure that
                                                                     the engine starts.

                                                                                                   62

| 62 63 64 65 66 67 68 69 70 71 72 |