Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-11-76
P. 45

    UF3Y11E0.book  Page 40  Tuesday, May 23, 2017  9:23 AM

                                                                     Instrument operation

                            The hour meter and voltmeter are displayed  If the battery voltage has dropped significant-
                            alternately at 3-second intervals.    ly, “Lo” is displayed on the voltmeter, and all
                                                                  other display segments  of the information
                                                   1
                                                                  display turn off. If the battery voltage has ris-
                                                                  en significantly, “HI” is displayed. If “Lo” or
                                                                  “HI” is displayed, immediately return to shore
                                                                  and have a Yamaha dealer service the water-
                                                                  craft.
                                                                                         1

                              1 Hour meter and voltmeter
                            TIP:
                            If the engine is stopped after the check en-
                            gine warning is activated, the hour meter and
                            error code will be displayed alternately at 3-
                            second intervals.
                                                                   1 Voltmeter
                            Hour meter
                                                                  EJU37272
                            The hour meter shows the total number of
                                                                  Fuel level meter
                            hours that the engine has been running since  The fuel level meter shows the amount of fuel
                            the watercraft was new.               remaining in the fuel tank. The amount of re-
                                                   1              maining fuel is shown using four display seg-
                                                                  ments, which disappear one at a time as the
                                                                  fuel level decreases.
                                                                  TIP:
                                                                  The accuracy of  the  fuel  level meter varies
                                                                  depending on the operating conditions. Use
                                                                  this function as a reference only.

                                                                      1
                              1 Hour meter

                            TIP:
                            The elapsed time will be kept even if the bat-
                            tery terminals have been disconnected.
                            Voltmeter
                            The voltmeter shows the battery voltage.
                            When the battery voltage is normal, the volt-
                            meter displays approximately 12 volts.  1 Fuel level meter

                                                                                                   40

| 40 41 42 43 44 45 46 47 48 49 50 |