Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-11-76
P. 52

    UF3Y11E0.book  Page 47  Tuesday, May 23, 2017  9:23 AM

                            Equipment operation

                            To open the glove compartment:        To close the glove compartment:
                            Pull the  glove  compartment latch up, and  Push the lid down to securely lock it in place.
                            then lift up the lid.

                                                         1

                                                                  EJU44491
                              1 Glove compartment latch           Seat storage compartment
                                                                  The seat storage compartment is located un-
                                                                  der the seat. (See page 43 for seat removal
                                                                  and installation procedures.)
                                                                                  1

                                                        1

                              1 Glove compartment

                              Glove compartment:
                                Capacity:                          1 Seat storage compartment
                                  14.0 L (3.7 US gal, 3.1 Imp.gal)
                                Load limit:                         Seat storage compartment:
                                  3.0 kg (7 lb)                       Capacity:
                                                                        8.0 L (2.1 US gal, 1.8 Imp.gal)
                                                                      Load limit:
                                                                        3.0 kg (7 lb)

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |