Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-11-76
P. 72

    UF3Y11E0.book  Page 67  Tuesday, May 23, 2017  9:23 AM

                            Operation

                            EJU40212                              EJU43580
                            Riding position                       Starting the engine on water
                            Operator riding position              EWJ01531
                            The operator should grip the handlebars firm-  WARNING
                            ly with both hands and sit astride the seat  Do not apply throttle when anyone is at the
                            with both feet on the floor of the footwell.  rear of the watercraft. Turn the engine off
                                                                  or keep it at idle. Water and debris exiting
                                                                  the jet thrust nozzle can cause severe in-
                                                                  jury.

                                                                  To start the engine:
                                                                  (1) Move the  watercraft to an  area  that is
                                                                     free from weeds and debris, and has a
                                                                     water depth of at least 60 cm (2 ft) from
                                                                     the bottom of the watercraft. NOTICE:
                                                                     Never run the engine in water that is
                                                                     less than 60 cm (2 ft) deep from the
                            Passenger riding position
                                                                     bottom  of the watercraft, otherwise
                            The passenger(s) should hold on firmly, either
                                                                     pebbles or sand could be sucked into
                            to the person in front of them or to the hand-
                                                                     the jet intake, causing impeller dam-
                            grip provided, and sit astride the seat with
                                                                     age and engine overheating. [ECJ00473]
                            their feet on the floor of the footwell. Never al-
                            low a passenger to ride in front of the opera-
                            tor. (See page 17 for information on the riding
                            position when pulling a wakeboarder or wa-
                            ter-skier.)

                                                                  (2) Attach the engine shut-off cord (lanyard)
                                                                     to your left wrist, and then attach the clip
                                                                     to the engine shut-off switch. (See page
                                                                     30 for information on operating the en-
                                                                     gine shut-off switch.) WARNING! Check
                            EJU32803
                            Launching the watercraft                 that the engine shut-off cord (lanyard)
                            When launching the watercraft,  make  sure  is attached  correctly. If the engine
                            that there are no obstacles around you.  shut-off cord (lanyard) is not attached
                            If the  watercraft is launched from a  trailer,  correctly, it may not pull free when the
                            someone should  make sure that waves do  operator falls off, allowing the water-
                            not push the watercraft into the trailer.

                            67

| 67 68 69 70 71 72 73 74 75 76 77 |