Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 91 - LIT-18626-11-76
P. 91

    UF3Y11E0.book  Page 86  Tuesday, May 23, 2017  9:23 AM

                                                                           Care and storage

                                engine is hot. The sprayed substance
                                or propellants could catch fire. [EWJ00262]

                                        1

                              1 Intake opening
                            (5) Place the air filter case cover in its origi-
                                nal position, and then fit the hooks onto
                                the cover.
                            TIP:
                            Make sure that the air filter case cover is se-
                            curely installed.
                            (6) Fasten the fuel hose to the holder using
                                the plastic tie.
                            (7) Make sure that the area around the wa-
                                tercraft is clear, and then start the engine
                                in a well-ventilated area and let it run at
                                idle for 15 seconds. (See page 30 for in-
                                formation on starting the engine.)
                            (8) Stop the engine.
                            (9) Securely install the fire extinguisher hold-
                                er and seat in their original positions.

                                                                                                   86

| 86 87 88 89 90 91 92 93 94 95 96 |