Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-11-76
P. 66

    UF3Y11E0.book  Page 61  Tuesday, May 23, 2017  9:23 AM

                            Pre-operation checks

                            right and left fully turned positions of the jet  Operate the shift lever several times to make
                            thrust nozzle.                        sure that operation is smooth throughout the
                                                                  whole range. Also, make sure that the reverse
                                                                  gate moves up and down according to the
                                                                  operation of the shift lever and that the gate
                                                                  makes contact with the stoppers. (See page
                                                                  34 for reverse system operation.)

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                Maximum 5 mm (0.20 in)
                            EJU32636
                            Reverse system checks (EX Sport)                              1
                            EWJ00032
                                 WARNING                           1 Stopper
                            Do not touch  the  reverse  gate while the  EJU43213
                            shift lever is being operated, otherwise  RiDE lever checks (EX Deluxe)
                                                                  Operate the RiDE lever several times to make
                            you could be pinched.
                                                                  sure that operation is smooth throughout the

                            61

| 61 62 63 64 65 66 67 68 69 70 71 |