Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-11-76
P. 73

    UF3Y11E0.book  Page 68  Tuesday, May 23, 2017  9:23 AM

                                                                                      Operation

                                craft to continue to run and cause an  to avoid. A collision could result in severe
                                accident. [EWJ00582]              injury or death. [EWJ00602]
                                                2
                                            1

                                                        3

                              1 Clip
                                                                  EJU32873
                              2 Engine shut-off switch            Leaving the watercraft
                              3 Engine shut-off cord (lanyard)    If leaving the watercraft, remove the clip from
                            (3) With the throttle lever released, push the  the  engine shut-off switch  to prevent acci-
                                start  switch (green  button) to start  the  dental starting or unauthorized operation by
                                engine. (See page 30 for information on  children or others.
                                operating the start switch.)

                                                                  EJU44361
                                                                  Operating the watercraft
                            EJU32863                              EX:
                            Stopping the engine
                                                                  When the  engine is running, the  watercraft
                            Release the throttle lever, and then push the
                                                                  will move forward at trolling speed even if the
                            engine stop switch (red button) to stop the
                            engine.  WARNING!  You need throttle  to
                            steer. Shutting  the engine off can  cause
                            you to hit an obstacle you are attempting

                                                                                                   68

| 68 69 70 71 72 73 74 75 76 77 78 |