Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 61 - LIT-18626-11-76
P. 61

    UF3Y11E0.book  Page 56  Tuesday, May 23, 2017  9:23 AM

                                                                    Pre-operation checks

                            EJU31982

                            EWJ00412
                                 WARNING
                            Failure to inspect or maintain the watercraft properly increases the possibility of an ac-
                            cident or damage to the watercraft. Do not operate the watercraft if you find any prob-
                            lem. If a problem cannot be corrected by the procedures provided in this manual, have
                            the watercraft inspected by a Yamaha dealer.

                            EJU41234
                            Pre-operation checklist
                            Before using this watercraft, be sure to perform the checks in the following checklist.
                                      ITEM                         ROUTINE                   PAGE
                             PRE-LAUNCH CHECKS
                                                    Ventilate the engine compartment.
                             Engine compartment                                               58
                                                    Check inside the engine compartment for damage.
                                                    Check the fuel system for leakage.
                             Fuel system                                                      58
                                                    Check the fuel level in the fuel tank.
                             Water separator        Check the water separator for water.      59
                             Engine unit            Check the exterior of the engine unit for damage.  59
                             Engine oil level       Check the engine oil level.               59
                             Bilge water            Check the engine compartment for bilge water.  59
                             Battery                Check the battery connections and electrolyte level.  59
                             Steering system        Check the steering system for proper operation.  60
                             Reverse system (EX Sport)  Check the reverse system for proper operation.  61
                             RiDE lever (EX Deluxe)  Check the RiDE lever for proper operation.  61
                             Throttle lever         Check the throttle lever for proper operation.  62
                             Engine shut-off cord (lan-  Check the engine shut-off cord (lanyard) for dam-  62
                             yard)                  age.
                                                    Check the start switch, engine stop switch, and en-
                             Switches                                                         62
                                                    gine shut-off switch for proper operation.
                                                    Check the storage compartments for damage and
                             Storage compartments                                             63
                                                    water.
                             Fire extinguisher holder  Check the fire extinguisher holder for damage.  63
                             Fire extinguisher      Check the condition of the fire extinguisher.  63
                                                    Check that safety equipment meeting the applica-
                             Safety equipment                                                 63
                                                    ble regulations is on board.
                             Hull and deck          Check the hull and deck for damage.       63
                             Jet intake             Check the jet intake for damage and clogging.  63
                             Jet thrust nozzle and re-  Check the jet thrust nozzle and reverse gate for
                             verse gate (EX Sport / EX   damage.                              63
                             Deluxe)
                                                    Check the stern drain plugs for damage and foreign
                             Stern drain plugs                                                63
                                                    material and check that they are securely installed.

                                                                                                   56

| 56 57 58 59 60 61 62 63 64 65 66 |