Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 79 - LIT-18626-11-76
P. 79

    UF3Y11E0.book  Page 74  Tuesday, May 23, 2017  9:23 AM

                                                                                      Operation

                            bles or sand could be sucked into the jet  (2) Pull yourself up to a kneeling position on
                            intake, causing impeller damage and en-  the boarding platform, and then move to
                            gine overheating. [ECJ00473]             the seat and sit astride.

                                         60 cm (2 ft)

                            TIP:                                  (3) Attach the engine shut-off cord (lanyard)
                                                                     to your left wrist, and then attach the clip
                            EX Sport /  EX Deluxe: This watercraft is
                                                                     to the engine shut-off switch.
                            equipped with a reboarding step, which can
                                                                  (4) Grip the handlebars with both hands and
                            be lowered and used to assist in reboarding.
                                                                     place both feet on the floor of the foot-
                            (See page 44 for information on operating the
                                                                     well.
                            reboarding step.)
                            EJU36354
                            Boarding alone
                            (1) From  the rear of the  watercraft, place
                                both hands on the boarding platform,
                                pull yourself up, and  then  grasp  the
                                handgrip with one hand.

                                                                  (5) Look  in all directions, start  the  engine,
                                                                     and then start off slowly.
                                                                  EJU43260
                                                                  Boarding with passenger(s)
                                                                  EWJ01800
                                                                      WARNING
                                                                   Severe internal injuries can occur if wa-
                                                                   ter is forced into body cavities as a re-
                                                                   sult of being near the jet thrust nozzle.
                                                                   Do not start the engine until the passen-
                                                                   gers are  seated with  their feet on the
                                                                   floor of the footwell and are securely

                                                                                                   74

| 74 75 76 77 78 79 80 81 82 83 84 |