Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-11-76
P. 48

    UF3Y11E0.book  Page 43  Tuesday, May 23, 2017  9:23 AM

                            Equipment operation

                            EJU40334                              To install the seat:
                                        Equipment
                                                                  (1) Insert the projection on the front of the
                            EJU44600
                            Seat                                     seat into the stay on the deck.
                            The seat is removable.
                            Remove  the seat to access the fire extin-
                            guisher holder, seat  storage compartment,
                            and engine compartment.
                            To remove the seat:
                            (1) Pull the seat latch up, and then lift up the
                                rear of the seat.

                                                                  (2) Push the rear of the seat down to secure-
                                                            1        ly lock it in place.

                              1 Seat latch
                            (2) Pull the seat rearward and remove it.

                                                                  EJU31364
                                                                  Handgrip
                                                                  The handgrip is used when boarding the wa-
                                                                  tercraft from the water and when the spotter
                                                                  is facing rearward. WARNING! Do not use
                                                                  the handgrip to lift the watercraft.  The
                                                                  handgrip is not  designed to support the
                                                                  watercraft’s weight. If the handgrip

                            43

| 43 44 45 46 47 48 49 50 51 52 53 |