Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-11-76
P. 51

    UF3Y11E0.book  Page 46  Tuesday, May 23, 2017  9:23 AM

                                                                     Equipment operation

                            To open the bow storage compartment:  To close the bow storage compartment:
                            Unhook the hood latches, and then lift up the  Return the hood to its original position, and
                            rear of the hood.                     then hook the hood latches to secure it in pla-
                                                                  ce.

                                                         1
                                                                                               1

                              1 Hood latch
                                                                   1 Hood latch
                                                                  EJU43781
                                                                  Glove compartment
                                                                  The glove compartment is located in front of
                               1                                  the seat.

                              1 Bow storage compartment

                              Bow storage compartment:
                                Capacity:
                                  7.0 L (1.8 US gal, 1.5 Imp.gal)
                                Load limit:
                                  2.0 kg (4 lb)

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |