Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 21 - LIT-18626-11-76
P. 21

    UF3Y11E0.book  Page 16  Tuesday, May 23, 2017  9:23 AM

                                                                         Safety information

                             EX Sport: Do not use the reverse function  sure that there are no obstacles or people
                              to slow down or stop the watercraft as it  behind you before shifting into reverse.
                              could cause you to lose control, be eject-   Keep away from the intake grate while the
                              ed, or impact the handlebars.        engine is on. Items such as long hair, loose
                              This could increase the risk of back/spinal  clothing, or PFD straps can become entan-
                              injury (paralysis), facial injuries, and broken  gled in moving parts, resulting in severe in-
                              legs, ankles, and other bones. You could  jury or drowning.
                              also damage the shift mechanism.     Never insert any object into the jet thrust
                             EX Sport: Reverse  can be used to slow  nozzle while the engine is running. Severe
                              down or stop during slow-speed maneu-  injury or death could result from coming in
                              vering, such  as when docking. Once  the  contact with the rotating parts of the jet
                              engine is idling, shift into reverse and grad-  pump.
                              ually increase engine speed. Make sure
                              that there are no obstacles or people be-
                              hind you before shifting into reverse.
                             EX Deluxe: This watercraft is water-jet pro-
                              pelled. The jet pump is directly connected
                              to the engine. This means that jet thrust will                     2
                              produce some  movement whenever  the
                              engine is running and the “F” (forward) or                 1
                              “R” (reverse)  shift  indicator is displayed.
                              When the “N” (neutral) shift indicator is dis-
                              played, the forward and reverse thrust are  1 Intake grate
                                                                   2 Jet thrust nozzle
                              balanced to help keep the watercraft from
                              moving in either direction, although some   Stop the engine and remove the clip from
                              movement may occur.                  the engine shut-off switch before removing
                                                                   any debris or weeds, which may have col-
                                         1
                                                                   lected around the jet intake.
                                                                                         2

                                                                                              1

                              1 “N” (Neutral position)
                             EX Deluxe: To avoid  rear-end collisions
                              while operating the watercraft, check be-  1 Clip
                                                                   2 Engine shut-off switch
                              hind you before using the RiDE lever to
                              slow  down or stop the watercraft. Make

                                                                                                   16

| 16 17 18 19 20 21 22 23 24 25 26 |