Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 89 - LIT-18626-11-76
P. 89

    UF3Y11E0.book  Page 84  Tuesday, May 23, 2017  9:23 AM

                                                                           Care and storage

                            EJU33493                               Steering cable (jet thrust nozzle end)
                                   Long-term storage
                            EWJ00331
                                 WARNING
                            Always place the watercraft upright in a
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            Storage for long periods of time, such as win-
                            ter storage, requires preventive maintenance
                            to ensure against deterioration. It is advisable   EX Sport: Shift cable (reverse gate end) and
                            to have the watercraft serviced by a Yamaha  ball joint
                            dealer prior to storage.
                            However,  the following  procedures can be
                            performed easily by the owner.
                            EJU40256
                            Cleaning
                            (1) Flush the cooling water passages. (See
                                page 80 for information on flushing the
                                cooling water passages.)
                            TIP:
                            If you will be storing the watercraft for a pro-
                            longed period, such as winter storage, top off
                            the fuel tank with fresh gasoline and add one
                            ounce of Yamalube Fuel Stabilizer & Condi-
                            tioner Plus to each gallon of fuel in the fuel
                            tank before starting the engine.
                            (2) Clean the watercraft. (See page 81 for in-  TIP:
                                formation on cleaning the watercraft.)  Disconnect the shift cable from the ball joint
                                Wax the  hull with a non-abrasive wax  before lubricating.
                                such as Yamalube Professional Polish.
                            EJU44960
                            Lubrication
                            To  keep  moving parts sliding or rotating
                            smoothly, lubricate them with water-resistant
                            grease.
                              Recommended water-resistant grease:
                                YAMALUBE MARINE GREASE

                                                                                                   84

| 84 85 86 87 88 89 90 91 92 93 94 |