Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-11-76
P. 78

    UF3Y11E0.book  Page 73  Tuesday, May 23, 2017  9:23 AM

                            Operation

                            Operating in reverse (EX Deluxe)      current location. (See page 34 for shift sys-
                            When the RiDE lever is squeezed, the “R” (re-  tem operation procedures.)
                            verse) shift indicator will be displayed and the   1
                            watercraft will move in reverse. (See page 34
                            for shift system operation procedures.)
                                         1

                                                                   1 “N” (Neutral position)

                              1 “R” (Reverse position)

                                                                  EJU36087
                                                                  Boarding the watercraft
                                                                  EWJ01112
                                                                      WARNING
                            Make sure that there are no obstacles or peo-
                                                                  Be sure the operator and any passengers
                            ple behind you before shifting into reverse.
                                                                  have practiced boarding from the water
                            TIP:                                  while still close to shore before riding. A
                            This model is equipped with a function which  person who has made many unsuccessful
                            limits the engine speed in reverse.   attempts to get back on the watercraft
                            Operating in neutral (EX Deluxe)      may become fatigued and suffer from ex-
                            When the RiDE lever is squeezed lightly and
                                                                  posure, increasing the  risk of injury and
                            released, the “N” (neutral) shift indicator will
                                                                  drowning.
                            be displayed and the watercraft will stop in its
                                                                  Board the watercraft in water free from
                                                                  weeds and debris and at least 60 cm (2 ft)
                                                                  deep  from the bottom of  the watercraft.
                                                                  NOTICE: Never run the engine in water
                                                                  that is less than 60 cm (2 ft) deep from the
                                                                  bottom of the watercraft, otherwise peb-

                            73

| 73 74 75 76 77 78 79 80 81 82 83 |