Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-11-76
P. 80

    UF3Y11E0.book  Page 75  Tuesday, May 23, 2017  9:23 AM

                            Operation

                              holding on to the person in front of them  (4) Have the first passenger board using the
                              or to the handgrip provided.           same procedure as the operator, place
                             Before boarding the watercraft, make   their feet on the floor of the footwell, and
                              sure that the engine is stopped. If the  securely hold on to the operator.
                              engine is running, the reverse gate may
                              move down  and a  person boarding
                              could be pinched.

                            The heavier the total weight of the operator
                            and passenger(s), the more difficult it will be
                            to balance the watercraft. Do not operate the
                            watercraft when the total weight exceeds 220
                            kg (486 lb) including any cargo.
                            To board with passenger(s):
                            (1) Board as noted in the previous section
                                                                  (5) Have the  second passenger follow the
                                “Boarding alone”.
                                                                     same procedure. When the second pas-
                                                                     senger is boarding, try to  balance  the
                                                                     watercraft together with the first passen-
                                                                     ger.

                            (2) Grip the handlebars with both hands and
                                place both feet on the floor of the foot-
                                well.
                            (3) Have the first passenger move to the rear
                                                                  (6) Make sure that  the passenger(s)  have
                                of the watercraft.
                                                                     their feet on the floor of the footwell and

                            75

| 75 76 77 78 79 80 81 82 83 84 85 |