Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-11-76
P. 69

    UF3Y11E0.book  Page 64  Tuesday, May 23, 2017  9:23 AM

                                                                    Pre-operation checks

                            flood the engine compartment and cause  EJU40146
                                                                  Post-launch checks
                            the watercraft to submerge. [ECJ00363]
                                                                  Perform the post-launch checks in the pre-
                                                                  operation checklist while the watercraft is in
                                                                  the water and the engine is running.
                                                                  To perform the post-launch checks:
                                                                  (1) Launch the watercraft. (See page 67 for
                                                                     information on launching the watercraft.)
                                                                  (2) Perform the checks and make sure that
                                                                     there are no malfunctioning items or oth-
                                       2                             er problems.
                                                                  EJU40553
                                       1                          Cooling water pilot outlet check
                              1 Stern drain plug                  Make sure that water is discharged from the
                              2 O-ring
                                                                  cooling water pilot outlet while the engine is
                            Securely install the stern drain plugs by tight-  running. (See page 32 for information on the
                            ening them until they stop.           cooling water pilot outlet.)

                                           1

                              1 Stern drain plug                  EJU32715
                                                                  Multifunction information center check
                            EJU44640
                            Hood check                            Make sure that the multifunction information
                            Close the hood, hook the hood latches, and  center operates properly. (See page 38 for in-
                            check that the hood is securely closed.  formation on proper operation of the multi-
                                                                  function information center.)

                                                         1

                              1 Hood latch

                                                                                                   64

| 64 65 66 67 68 69 70 71 72 73 74 |