Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 127 - LIT-18626-11-77
P. 127

    SportsBoat_F3M12.book  Page 121  Monday, June 12, 2017  11:53 AM

                                                                           Trouble recovery

                            (2) While pushing both sides of the fuse box  190 FSH
                                cover inward, pull the cover toward the
                                bow and remove it.

                                                                                               1
                                                                        2

                                                    1

                                                                                       3
                                                                  1  Fuse holder
                                                                  2  Accessory fuse
                                                                  3  Bilge fuse
                            1  Fuse box cover
                                                                  190 FSH Sport/190 FSH Deluxe
                                12 3      4       5     6

                                                                                                 2

                                                                                                 3

                                                                             1
                                         8       7

                            1  Electronic throttle valve fuse     1  Fuse holder
                            2  Fuel pump fuse                     2  Accessory fuse
                            3  Main relay drive fuse              3  Bilge fuse
                            4  Main fuse
                            5  Fuse puller                        (4) Replace the blown  fuse with  the  spare
                            6  Battery fuse                          fuse of the correct amperage by using the
                            7  Spare fuse
                                                                     fuse puller.
                            8  Unused fuse
                            (3) When replacing an accessory fuse and
                                bilge fuse, remove the fuse holder. (See
                                page 60 for battery compartment opening
                                and closing procedures.)

                                                                                                 121

| 122 123 124 125 126 127 128 129 130 131 132 |