Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 120 - LIT-18626-11-77
P. 120

    SportsBoat_F3M12.book  Page 114  Monday, June 12, 2017  11:53 AM

                            Specifications

                                                         Specifications

                                            ITEM                              Specification
                             Boat capacity
                             Maximum people on board             8 person
                             Maximum load capacity               658 kg (1450 lb)
                             Dimensions and weight
                             Length                              5840 mm (229.9 in)
                             Beam                                2440 mm (96.1 in)
                             Height                              2720 mm (107.1 in) (190 FSH Sport)
                                                                 1980 mm (78.0 in) (190 FSH Deluxe/190 FSH)
                             Draft                               380 mm (15.0 in) (190 FSH Sport)
                                                                 360 mm (14.2 in) (190 FSH Deluxe)
                                                                 350 mm (13.8 in) (190 FSH)
                             Dry weight                          1068 kg (2355 lb) (190 FSH Sport)
                                                                 1023 kg (2255 lb) (190 FSH Deluxe)
                                                                 980 kg (2161 lb) (190 FSH)
                             Performance
                             Maximum fuel consumption            48.5 L/h (12.8 US gal/h, 10.7 Imp.gal/h)
                             Cruising range at full throttle     2.34 hour
                             Trolling speed                      1300 ±100 r/min
                             Engine
                             Number of engines                   1
                             Engine type                         Liquid cooled 4-stroke, DOHC
                             Number of cylinders                 4
                             Engine displacement                 1812 cm 3
                             Bore × stroke                       86.0 × 78.0 mm (3.39 × 3.07 in)
                             Compression ratio                   11.0 : 1
                             Valve clearance-intake (cold)       0.14–0.23 mm (0.0055–0.0091 in)
                             Valve clearance-exhaust (cold)      0.28–0.37 mm (0.0110–0.0146 in)
                             Lubrication system                  Wet sump
                             Cooling system                      Water
                             Starting system                     Electric
                             Ignition system                     T.C.I.
                             Spark plug (NGK)                    LFR6A
                             Spark plug gap                      0.8–0.9 mm (0.031–0.035 in)
                             Battery capacity                    12 V, 85 Ah
                             Charging system                     Flywheel magneto

                            114

| 115 116 117 118 119 120 121 122 123 124 125 |