Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-11-77
P. 67

    UF3P11E0.book  Page 62  Wednesday, June 14, 2017  11:35 AM

                                                                    Pre-operation checks

                                      ITEM                         ROUTINE                   PAGE
                             Hood                   Check that the hood is securely closed.   69
                             Front and rear seats   Check that the seats are securely installed.  47
                             POST-LAUNCH CHECKS
                                                    Check that water is discharged from the port (left)
                             Cooling water pilot outlet  cooling water pilot outlet while the engine is run-  69
                                                    ning.
                             Multifunction information   Check the multifunction information center for prop-  69
                             center                 er operation.
                             Shift system           Check the shift system for proper operation.  69
                             Trim indicator         Check the trim indicator for proper operation.  70
                             Engine idling speed    Check the engine idling speed.            70
                            TIP:
                            To ensure safety and reliability, pre-operation checks should be made each time the water-
                            craft is used.

                                                                                                   62

| 62 63 64 65 66 67 68 69 70 71 72 |