Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 117 - LIT-18626-11-77
P. 117

    SportsBoat_F3M12.book  Page 111  Monday, June 12, 2017  11:53 AM

                                                                                  Maintenance

                            Periodic maintenance chart
                            The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
                            Yamaha dealer perform the checks in the following chart. However, maintenance may need to
                            be performed more frequently depending on your operating conditions. If you have any ques-
                            tions, consult a Yamaha dealer.
                            This “ √ ” mark indicates items to be checked and serviced by a Yamaha dealer.
                                                                           Initial  Thereafter every
                                                                                   50    100    200
                                    Item                Operation                 hours   hours   hours
                                                                            10
                                                                           hours  or 12   or 12   or 24
                                                                                 months  months  months
                                                                                   *1     *1     *1
                             Fuel hoses, clamps,   Check for damage, and check con-
                             canister, and check   nections and tightening of clamps      √
                             valve
                                               Check cap for damage, and check
                             Fuel filler cap                                              √
                                               seal for cracks and deformation
                             Fuel tank         Check installation            √            √
                             Main switch and en-  Check operation            √            √
                             gine shut-off switch
                             Battery (190 FSH)/  Check state of charge and termi-
                             Batteries         nals, and check for broken battery         √
                             (190 FSH Sport/   straps
                             190 FSH Deluxe)
                             Battery leads     Check terminals                            √
                             Battery switch
                             (190 FSH)/
                             Battery switches   Check operation              √            √
                             (190 FSH Sport/
                             190 FSH Deluxe)
                             Meters (after com-
                             pleting the pre-opera-  Check lighting          √            √
                             tion checks)
                             Neutral switch    Check operation               √            √
                             Hatch interlock
                             switch (wet storage   Check operation           √            √
                             compartment)
                             Blower            Check operation               √            √
                             Horn              Check operation               √            √
                             Navigation lights  Check lighting               √            √
                                               Check for water discharge by auto-
                                               matic operation, clean filter, check
                             Electric bilge pump                                          √
                                               hoses for damage, and check tight-
                                               ening of clamps
                             Other electrical com-  Check operation of livewell, jet   √  √
                             ponents           wash, stereo, and other components
                             Steering master   Check operation and tilting mecha-  √      √
                             ASSY              nism, and check for looseness

                                                                                                 111

| 112 113 114 115 116 117 118 119 120 121 122 |