Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 121 - LIT-18626-11-77
P. 121

    SportsBoat_F3M12.book  Page 115  Monday, June 12, 2017  11:53 AM

                                                                                Specifications

                                            ITEM                              Specification
                             Drive unit
                             Propulsion system                   Jet pump
                             Jet pump type                       Axial flow, single stage
                             Impeller rotation                   Counterclockwise
                             Pitch angle                         14.0°
                             Transmission                        Direct drive from engine
                             Jet thrust nozzle angle             23.0+23.0°
                             Fuel and oil
                             Recommended fuel                    Regular unleaded gasoline
                             Minimum octane rating (PON)         86
                             Minimum octane rating (RON)         90
                             Fuel tank total capacity            114 L (30.0 US gal, 25.0 Imp.gal)
                             Recommended engine oil              YAMALUBE 4W or 4-stroke motor oil
                             Recommended engine oil type SAE     SAE 10W-30, 10W-40, 20W-40, 20W-50
                             Recommended engine oil grade API    API SG, SH, SJ, SL
                             Engine oil total quantity           5.3 L (5.60 US qt, 4.66 Imp.qt)
                             Engine oil quantity without oil filter replacement  3.5 L (3.70 US qt, 3.08 Imp.qt)
                             Engine oil quantity with oil filter replacement  3.6 L (3.81 US qt, 3.17 Imp.qt)
                             Fuse amperage
                             Electronic throttle valve fuse      10 A
                             Fuel pump fuse                      10 A
                             Main relay drive fuse               10 A
                             Main fuse                           20 A
                             Battery fuse                        30 A
                             Accessory fuse                      20 A
                             Bilge fuse                          3 A

                                                                                                 115

| 116 117 118 119 120 121 122 123 124 125 126 |