Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-11-77
P. 78

    UF3P11E0.book  Page 73  Wednesday, June 14, 2017  11:35 AM

                            Operation

                                is attached  correctly. If the engine  to avoid. A collision could result in severe
                                shut-off cord (lanyard) is not attached  injury or death. [EWJ00602]
                                correctly, it may not pull free when the
                                operator falls off, allowing the water-
                                craft to continue to run and cause an
                                accident. [EWJ00582]
                                                     1   2

                                                                  EJU32873
                                                                  Leaving the watercraft
                                                  3               If leaving the watercraft, remove the clip from
                                                                  the  engine shut-off switch  to prevent acci-
                              1 Clip                              dental starting or unauthorized operation by
                              2 Engine shut-off switch            children or others.
                              3 Engine shut-off cord (lanyard)
                            (4) With the throttle lever released, push the
                                start  switch (green  button) to start  the
                                engine. (See page 32 for information on
                                operating the start switch.)

                                                                  EJU43411
                                                                  Operating the watercraft
                                                                  When the throttle lever is squeezed, the “F”
                                                                  (forward) shift indicator will be displayed and
                                                                  the watercraft will move forward. While the
                                                                  “F” (forward) shift indicator is displayed, the
                            EJU32863                              watercraft will move forward at trolling speed
                            Stopping the engine
                            Release the throttle lever, and then push the  even if the throttle lever is in the fully closed
                            engine stop switch (red button) to stop the
                            engine.  WARNING!  You need throttle  to
                            steer. Shutting  the engine off can  cause
                            you to hit an obstacle you are attempting

                            73

| 73 74 75 76 77 78 79 80 81 82 83 |