Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 119 - LIT-18626-11-77
P. 119

    SportsBoat_F3M12.book  Page 113  Monday, June 12, 2017  11:53 AM

                                                                                  Maintenance

                                                                           Initial  Thereafter every
                                                                                   50    100    200
                                    Item                Operation                 hours   hours   hours
                                                                            10
                                                                           hours  or 12   or 12   or 24
                                                                                 months  months  months
                                                                                   *1     *1     *1
                                               Check for bends, damage, and for-
                             Impeller                                        √            √
                                               eign material
                             Impeller duct     Check and lubricate                        √
                             Jet thrust nozzle  Check movement, and lubricate             √
                             Intermediate housing  Lubricate                              √
                             Anode (jet pump unit)  Check for corrosion                   √
                            *1: Whichever comes first.
                            *2: Check every 200 hours.
                            Perform the pre-operation checks and post-operation checks before performing periodic main-
                            tenance.

                                                                                                 113

| 114 115 116 117 118 119 120 121 122 123 124 |