Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 125 - LIT-18626-11-77
P. 125

    SportsBoat_F3M12.book  Page 119  Monday, June 12, 2017  11:53 AM

                                                                           Trouble recovery

                                      1

                                                                                              1

                                                                        3
                                                                                            2

                            1  Access port cap                    1  “SET” mark
                                                                  2  Slot
                            (5) Remove any weeds or debris from the  3  Edge of the access port
                                drive shaft, impeller, pump housing, and
                                jet  thrust  nozzle. If you cannot  remove  (8) Check that the cap is perpendicular to the
                                the debris, consult a Yamaha Boat Deal-  centerline of  the boat. Pull the handle
                                er.                                  forcefully to make sure that the cap is
                            (6) To  reinstall  the access port cap, first  locked securely. If a strong pull will move
                                clean off any sand or other foreign matter  the access port cap, it is not locked se-
                                from  the cap or port surfaces.  Apply a  curely—the cap could be forced out by
                                light coat  of Yamalube Waterproof Ma-  water pressure during operation.
                                rine Grease (P/N: ACC-GREAS-10-CT),
                                if available, to the seal of the access port
                                cap. If grease is not available, apply the
                                grease during the post-operation checks.
                            (7) Insert the cap so that the “SET” mark is  1
                                aligned with the slot, and then while
                                pushing the handle turn the  cap  clock-
                                wise until the “SET” mark is aligned with
                                the edge of the access port.

                                                                  1  Perpendicular to the centerline of the boat

                                                                  (9) Close the rear platform hatch.
                                                                  NOTICE
                                                                  ● Be sure the access port  cap  is locked
                                                                   securely in place. Otherwise, the cap
                                                                   could be forced out of the access port
                                                                   by water pressure, causing loss of per-
                                                                   formance and possible damage.

                                                                                                 119

| 120 121 122 123 124 125 126 127 128 129 130 |